# ASCA interface update

  ASCA\_Ex(out\_folder, input\_file\_list)

Where out\_folder – is output folder name for debug output. There is no debug output if it is defined as “”.

input\_file\_list – list of input files for processing which contains the files-names of files that must be processed. ASCA parses the list according to the internal patterns as it is defined below:

\*.maggrid – magnetic grid

\*.mfp3 - magnetic fingerprint file

\*.wifigrid – wifi grid

\*.wifi3 - wifi fingerprint file

\*.blegrid – BLE grid

\*.ble3 - BLE fingerprint file

\*venue.json – venue settings file

\*mapN.geojson – one or more geojson-files with survey routs, where N – is physical floor number (one or more digits)

If any grid or fingerprint are not presented in list, then this fingerprint is not used for total coverage assessment.

There are no requirements for items sorting and order into this list.

\*.mfp4, \*.wifi4, \*.ble4 and other format-4 files are supposed to be supported in future